fabric 0.51 dcf 17 gsm

copy and paste the coordinates below into the manual editor on the myogtutorials.com pattern generator.
ensure that all other coordinates were overwritten.
click anywhere outside the manual editor text box to update the visualizer.
then, under display lengths, set the catenary cut curve depth to 0 cm/m.

{
  "apexAbsolute": {
    "x": 140,
    "y": 70,
    "z": 127
  },
  "baseCornersRelative": [
    {
      "rel_x": 0,
      "rel_y": 60,
      "z": 60
    },
    {
      "rel_x": 130,
      "rel_y": 0,
      "z": 10
    },
    {
      "rel_x": 130,
      "rel_y": -95,
      "z": 10
    },
    {
      "rel_x": -130,
      "rel_y": -95,
      "z": 10
    },
    {
      "rel_x": -130,
      "rel_y": 0,
      "z": 10
    }
  ]
}